{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"merged":[[0,0,0,6],[2,1,7,1],[8,1,16,1],[17,1,23,1],[24,1,28,1],[29,1,37,1],[38,1,40,1],[41,1,43,1],[46,3,46,4],[47,3,47,4]],"flags":["formulas_cached_only"]}
["广重集团生活污水处理站维护服务项目明细"]
["序号","分部","项目名称","数量","单位","维保方式","提供维保服务工作明细"]
[1,"一、废渣污泥清理","集水池废渣清理",50,"M3","承包方填写","承包方填写"]
[2,null,"调节池废渣污泥清理",50,"M3"]
[3,null,"厌氧池废渣污泥清理",250,"M3"]
[4,null,"好氧池废渣污泥清理",500,"M3"]
[5,null,"沉淀池废渣污泥清理",100,"M3"]
[6,null,"淤泥池废渣污泥清理",80,"M3"]
[7,"二、水系统","主提升泵（3相2KW）维护、保养",2,"台"]
[8,null,"备用提升泵（3相2.5KW）维护、保养",2,"台"]
[9,null,"提升软管DN90",20,"米"]
[10,null,"ABS转接头",2,"个"]
[11,null,"金属焊接止回阀DN90",4,"个"]
[12,null,"焊接流量调节阀DN90",1,"个"]
[13,null,"金属排水管DN90",50,"米"]
[14,null,"污泥池回水管DN100",15,"米"]
[15,null,"气提污泥管DN90",45,"米"]
[16,"三、电系统","PLC控制11回路立式电柜",1,"台"]
[17,null,"主、备提升泵电源电线4*4、保护套管",500,"米"]
[18,null,"液位控制器",4,"套"]
[19,null,"液位控制器电源线4*2.5、保护套管",500,"M3"]
[20,null,"污泥池电磁阀、电源线",1,"套"]
[21,null,"鼓风机电源",2,"组"]
[22,null,"二级分电箱",3,"套"]
[23,"四、空气系统","主、备4KW回转式罗茨鼓风机（使用年限已20年）",2,"台"]
[24,null,"DN100ABS主管",30,"米"]
[25,null,"沉淀池气提机",2,"套"]
[26,null,"气提管",50,"米"]
[27,null,"耗氧池曝气系统",500,"米"]
[28,"五、钢构件系统","好氧池填料钢构排架",160,"M2"]
[29,null,"沉淀池溢流堰",24,"米"]
[30,null,"沉淀池进水主管DN300",20,"米"]
[31,null,"沉淀池布水器",2,"套"]
[32,null,"污泥管",40,"米"]
[33,null,"下井爬梯",4,"套"]
[34,null,"花纹板井盖1.2*1.2",10,"个"]
[35,null,"集水井格栅",1,"套"]
[36,null,"厌氧池格栅支架",1,"套"]
[37,"六、药物","集水池",50,"M3"]
[38,null,"厌氧池",250,"M3"]
[39,null,"好氧池",500,"M3"]
[40,"七、取样监测","配合番禺区环境监测站月、季度监测",12,"次"]
[41,null,"配合生态环境管理部门以及第三方监测单位不定期监测","若干","次"]
[42,null,"自行监测",12,"次"]
[43,"八、协助","协助每年厂里的ISO外审，生态环境、安全生产监督、水务局、河长办等部门巡查工作","若干","次"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}